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	Supplemental Table 1. cCMV pooled prevalence per 1,000 live births: overall, maternal race/ethnicity-stratified, and maternal age group-stratified

	Maternal group
	Pooled prevalence (95% CI)

	Overalla
	4.7 (3.9–5.5)

	Race/ethnicity
	

	     Non-Hispanic White
	3.8 (2.4–5.6)

	     Non-Hispanic Black
	8.6 (6.5–10.0)

	     Hispanic
	3.5 (1.4–6.4)

	     Non-Hispanic Asian
	2.4 (0.6–5.6)

	     Non-Hispanic AIAN
	10.8 (1.9–26.8)

	Age group
	

	     ≤24 years
	7.2 (5.1–10.2)

	     25–29 years
	3.0 (2.5–3.6)

	     30–34 years
	3.5 (1.8–6.7)

	     ≥35 years
	2.5 (1.2–5.0)

	Here, study-specific prevalence included from Schleiss et al. includes both pre- and during-COVID-19 pandemic estimates (e.g., all published data). Results are similar to the main analysis, which only included pre-pandemic prevalence in the meta-analysis, obtained via study authors.

	aOverall indicates the pooled estimate using each study’s overall, non-stratified prevalence.




	Supplemental Table 2. National and state-specific cCMV infection prevalence per 1,000 live births, estimated number of infections, and estimated number of symptomatic cases, adjusted by maternal race/ethnicity, 2018–2022 

	
	2018
	2019
	2020
	2021
	2022

	
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)

	US
	4.6 
(3.0-7.3)
	17600 
(11500-27500)
	3170 
(2070-4960)
	4.6 
(3.0-7.3)
	17400 
(11400-27300)
	3130 
(2050-4910)
	4.7 
(3.0-7.3)
	16800 
(11000-26300)
	3030 
(1980-4730)
	4.6 
(3.0-7.2)
	17000 
(11100-26500)
	3050 
(1990-4780)
	4.6 
(3.0-7.3)
	16900 
(11000-26600)
	3050 
(1980-4790)

	AL
	5.6 
(4.1-7.5)
	300 
(200-400)
	60 
(40-80)
	5.6 
(4.2-7.5)
	300 
(200-400)
	60 
(40-80)
	5.6 
(4.1-7.5)
	300 
(200-400)
	60 
(40-80)
	5.5 
(4.0-7.4)
	300 
(200-400)
	60 
(40-80)
	5.4 
(4.0-7.4)
	300 
(200-400)
	60 
(40-80)

	AK
	5.1 
(2.5-11.8)
	100 
(0-100)
	60 
(30-120)
	5.1 
(2.5-11.9)
	60 
(30-120)
	10 
(0-20)
	5.1 
(2.6-11.8)
	50 
(30-120)
	10 
(0-20)
	5.1 
(2.5-11.7)
	50 
(30-110)
	10 
(0-20)
	5.1 
(2.5-11.7)
	50 
(30-110)
	10 
(0-20)

	AZ
	4.3 
(2.4-8.3)
	300 
(200-700)
	60 
(30-120)
	4.3 
(2.4-8.3)
	300 
(200-700)
	60 
(30-120)
	4.3 
(2.4-8.2)
	300 
(200-600)
	60 
(30-110)
	4.3 
(2.4-8.1)
	300 
(200-600)
	60 
(30-110)
	4.3 
(2.4-8.2)
	300 
(200-600)
	60 
(30-120)

	AR
	4.9 
(3.4-7.0)
	200 
(100-300)
	30 
(20-50)
	4.9 
(3.4-7.0)
	200 
(100-300)
	30 
(20-50)
	4.9 
(3.4-7.1)
	200 
(100-200)
	30 
(20-40)
	4.9 
(3.4-7.0)
	200 
(100-300)
	30 
(20-50)
	4.8 
(3.3-7.0)
	200 
(100-200)
	30 
(20-40)

	CA
	3.9 
(2.2-7.3)
	1800 
(1000-3300)
	320 
(180-590)
	3.9 
(2.2-7.3)
	1700 
(1000-3200)
	310 
(180-580)
	3.9 
(2.2-7.3)
	1700 
(900-3100)
	300 
(170-550)
	4.0 
(2.2-7.3)
	1700 
(900-3000)
	300 
(170-550)
	3.9 
(2.2-7.3)
	1600 
(900-3000)
	300 
(160-550)

	CO
	4.1 
(2.5-6.8)
	300 
(200-400)
	50 
(30-80)
	4.1 
(2.5-6.8)
	300 
(200-400)
	50 
(30-80)
	4.2 
(2.5-6.8)
	300 
(200-400)
	50 
(30-80)
	4.1 
(2.5-6.8)
	300 
(200-400)
	50 
(30-80)
	4.1 
(2.5-6.8)
	300 
(200-400)
	50 
(30-80)

	CT
	4.5 
(2.9-7.0)
	200 
(100-200)
	30 
(20-40)
	4.5 
(2.9-7.0)
	200 
(100-200)
	30 
(20-40)
	4.5 
(2.9-7.0)
	100 
(100-200)
	30 
(20-40)
	4.5 
(2.9-7.0)
	200 
(100-200)
	30 
(20-40)
	4.5 
(2.9-7.0)
	200 
(100-200)
	30 
(20-40)

	DE
	5.3 
(3.8-7.5)
	60 
(40-80)
	10 
(10-10)
	5.3 
(3.8-7.6)
	60 
(40-80)
	10 
(10-10)
	5.3 
(3.8-7.6)
	60 
(40-80)
	10 
(10-10)
	5.3 
(3.8-7.6)
	60 
(40-80)
	10 
(10-10)
	5.3 
(3.8-7.6)
	60 
(40-80)
	10 
(10-10)

	DC
	6.4 
(4.9-8.4)
	60 
(50-80)
	10 
(10-10)
	6.3 
(4.9-8.4)
	60 
(40-80)
	10 
(10-10)
	6.3 
(4.9-8.3)
	60 
(40-70)
	10 
(10-10)
	6.2 
(4.7-8.3)
	50 
(40-70)
	10 
(10-10)
	6.2 
(4.8-8.4)
	50 
(40-70)
	10 
(10-10)

	FL
	5.0 
(3.4-7.4)
	1100 
(800-1600)
	200 
(140-300)
	5.0 
(3.4-7.4)
	1100 
(800-1600)
	200 
(140-290)
	5.0 
(3.4-7.5)
	1000 
(700-1600)
	190 
(130-280)
	5.0 
(3.4-7.4)
	1100 
(700-1600)
	190
(130-290)
	5.0 
(3.4-7.5)
	1100 
(800-1700)
	200 
(140-300)

	GA
	5.8 
(4.3-7.8)
	700 
(500-1000)
	130 
(100-180)
	5.8 
(4.3-7.8)
	700 
(500-1000)
	130 
(100-180)
	5.8 
(4.3-7.9)
	700 
(500-1000)
	130 
(90-170)
	5.7 
(4.2-7.8)
	700 
(500-1000)
	130 
(90-180)
	5.7 
(4.2-7.8)
	700 
(500-1000)
	130 
(100-180)

	HI
	4.3 
(2.5-7.8)
	70 
(40-130)
	10 
(10-20)
	4.3 
(2.5-7.7)
	70 
(40-130)
	10 
(10-20)
	4.3 
(2.5-7.7)
	70 
(40-120)
	10 
(10-20)
	4.4 
(2.5-7.9)
	70 
(40-120)
	10 
(10-20)
	4.3 
(2.5-7.8)
	70 
(40-120)
	10 
(10-20)

	ID
	4.0 
(2.4-6.4)
	90 
(50-140)
	20 
(10-20)
	4.0 
(2.4-6.4)
	90 
(50-140)
	20 
(10-30)
	4.0 
(2.4-6.5)
	90 
(50-140)
	20 
(10-30)
	4.0 
(2.4-6.5)
	90 
(50-150)
	20 
(10-30)
	4.0 
(2.4-6.4)
	90 
(50-140)
	20 
(10-30)

	IL
	4.7 
(3.2-7.1)
	700 
(500-1000)
	120 
(80-190)
	4.7 
(3.2-7.1)
	700 
(400-1000)
	120 
(80-180)
	4.7 
(3.2-7.1)
	600 
(400-900)
	110 
(80-170)
	4.7 
(3.1-7.1)
	600 
(400-900)
	110 
(70-170)
	4.6
(3.1-7.1)
	600 
(400-900)
	110
(70-160)

	IN
	4.6 
(3.1-6.7)
	400 
(200-500)
	70 
(40-100)
	4.6 
(3.1-6.7)
	400 
(200-500)
	70 
(40-100)
	4.6 
(3.1-6.7)
	400 
(200-500)
	60 
(40-90)
	4.6 
(3.1-6.7)
	400 
(200-500)
	70 
(40-100)
	4.6 
(3.1-6.7)
	400 
(200-500)
	70 
(40-100)

	IA
	4.3 
(2.7-6.5)
	200 
(100-200)
	30 
(20-40)
	4.3 
(2.8-6.5)
	200 
(100-200)
	30 
(20-40)
	4.3 
(2.7-6.5)
	200 
(100-200)
	30 
(20-40)
	4.3 
(2.7-6.4)
	200 
(100-200)
	30 
(20-40)
	4.3 
(2.7-6.5)
	200 
(100-200)
	30 
(20-40)

	KS
	4.3 
(2.7-6.6)
	200 
(100-200)
	30 
(20-40)
	4.3 
(2.7-6.6)
	200 
(100-200)
	30 
(20-40)
	4.3 
(2.7-6.7)
	100 
(100-200)
	30 
(20-40)
	4.3 
(2.7-6.7)
	100 
(100-200)
	30 
(20-40)
	4.3 
(2.7-6.6)
	100 
(100-200)
	30 
(20-40)

	KY
	4.4 
(2.9-6.4)
	200 
(200-300)
	40 
(30-60)
	4.4 
(2.9-6.4)
	200 
(200-300)
	40 
(30-60)
	4.5 
(2.9-6.5)
	200 
(200-300)
	40 
(30-60)
	4.5 
(2.9-6.5)
	200 
(200-300)
	40 
(30-60)
	4.4 
(2.9-6.5)
	200 
(200-300)
	40 
(30-60)

	LA
	5.9 
(4.5-7.9)
	400 
(300-500)
	60 
(50-80)
	5.9 
(4.5-7.9)
	400 
(300-500)
	60 
(50-80)
	6.0 
(4.5-7.9)
	300 
(300-500)
	60 
(50-80)
	5.9 
(4.5-7.8)
	300 
(300-500)
	60 
(50-80)
	5.9 
(4.4-7.9)
	300 
(200-400)
	60 
(40-80)

	ME
	4.2 
(2.7-6.3)
	50 
(30-80)
	10 
(10-10)
	4.2 
(2.7-6.3)
	50 
(30-70)
	10 
(10-10)
	4.2 
(2.7-6.3)
	50 
(30-70)
	10 
(10-10)
	4.2 
(2.7-6.3)
	50 
(30-80)
	10 
(10-10)
	4.3 
(2.7-6.3)
	50 
(30-80)
	10 
(10-10)

	MD
	5.5 
(4.0-7.8)
	400 
(300-600)
	70 
(50-100)
	5.5 
(4.0-7.8)
	400 
(300-500)
	70 
(50-100)
	5.5 
(4.0-7.8)
	400 
(300-500)
	70 
(50-100)
	5.5 
(4.0-7.8)
	400 
(300-500)
	70 
(50-100)
	5.5 
(3.9-7.8)
	400
(300-500)
	70 
(50-100)

	MA
	4.3 
(2.8-6.8)
	300 
(200-500)
	50 
(30-90)
	4.3 
(2.7-6.9)
	300 
(200-500)
	50 
(30-90)
	4.3 
(2.7-6.9)
	300 
(200-500)
	50 
(30-80)
	4.3 
(2.7-6.8)
	300 
(200-500)
	50 
(30-90)
	4.4 
(2.8-6.9)
	300 
(200-500)
	50 
(30-90)

	MI
	4.9 
(3.4-7.0)
	500 
(400-800)
	100 
(70-140)
	4.9 
(3.4-7.0)
	500 
(400-800)
	100 
(70-140)
	4.9 
(3.4-7.0)
	500 
(400-700)
	90 
(60-130)
	4.9 
(3.4-7.0)
	500 
(400-700)
	90 
(60-130)
	4.9 
(3.3-7.0)
	500 
(300-700)
	90 
(60-130)

	MN
	4.6 
(3.0-7.1)
	300 
(200-500)
	60 
(40-90)
	4.6 
(3.0-7.1)
	300 
(200-500)
	50 
(40-80)
	4.6 
(3.0-7.2)
	300 
(200-500)
	50 
(30-80)
	4.6 
(3.0-7.1)
	300 
(200-500)
	50 
(30-80)
	4.6 
(3.0-7.1)
	300 
(200-500)
	50 
(30-80)

	MS
	6.2 
(4.8-8.1)
	200 
(200-300)
	40 
(30-50)
	6.2 
(4.9-8.1)
	200 
(200-300)
	40 
(30-50)
	6.2 
(4.8-8.1)
	200 
(200-300)
	40 
(30-50)
	6.2 
(4.8-8.0)
	200 
(200-300)
	40 
(30-50)
	6.1 
(4.7-8.0)
	200 
(200-300)
	40 
(30-50)

	MO
	4.8 
(3.2-6.8)
	300 
(200-500)
	60 
(40-90)
	4.8 
(3.2-6.8)
	300 
(200-500)
	60 
(40-90)
	4.8 
(3.2-6.8)
	300 
(200-500)
	60 
(40-80)
	4.7 
(3.2-6.8)
	300 
(200-500)
	60 
(40-80)
	4.7 
(3.2-6.8)
	300 
(200-500)
	60 
(40-80)

	MT
	4.5 
(2.4-8.8)
	50 
(30-100)
	10 
(10-20)
	4.5 
(2.4-8.8)
	50 
(30-100)
	10 
(0-20)
	4.5 
(2.4-8.7)
	50 
(30-90)
	10 
(0-20)
	4.4 
(2.4-8.3)
	50 
(30-90)
	10 
(0-20)
	4.4 
(2.4-8.4)
	50 
(30-90)
	10 
(0-20)

	NE
	4.3 
(2.7-6.9)
	100 
(100-200)
	20 
(10-30)
	4.3 
(2.7-6.9)
	100 
(100-200)
	20 
(10-30)
	4.3 
(2.7-6.9)
	100 
(100-200)
	20 
(10-30)
	4.3 
(2.6-6.8)
	100 
(100-200)
	20 
(10-30)
	4.3 
(2.7-6.9)
	100 
(100-200)
	20 
(10-30)

	NV
	4.5 
(2.8-7.5)
	200 
(100-300)
	30 
(20-50)
	4.5 
(2.8-7.5)
	200 
(100-300)
	30 
(20-50)
	4.6 
(2.9-7.6)
	200 
(100-300)
	30 
(20-50)
	4.6 
(2.9-7.5)
	200 
(100-300)
	30 
(20-50)
	4.6 
(2.9-7.6)
	200 
(100-300)
	30 
(20-50)

	NH
	4.0 
(2.4-6.0)
	50 
(30-70)
	10 
(10-10)
	4.0 
(2.4-6.1)
	50 
(30-70)
	10 
(10-10)
	4.0 
(2.5-6.1)
	50 
(30-70)
	10 
(10-10)
	4.0 
(2.4-6.0)
	50 
(30-80)
	10 
(10-10)
	4.0 
(2.5-6.1)
	50 
(30-70)
	10 
(10-10)

	NJ
	4.5 
(2.9-7.1)
	500 
(300-700)
	80 
(50-130)
	4.4 
(2.9-7.1)
	400
(300-700)
	80 
(50-130)
	4.5 
(2.9-7.1)
	400
(300-700)
	80 
(50-130)
	4.4 
(2.8-7.1)
	400 
(300-700)
	80 
(50-130)
	4.4 
(2.8-7.1)
	500 
(300-700)
	80 
(50-130)

	NM
	4.4 
(2.1-9.9)
	100 
(0-200)
	20 
(10-40)
	4.4 
(2.1-10.0)
	100 
(0-200)
	20 
(10-40)
	4.4 
(2.1-9.9)
	100 
(0-200)
	20 
(10-40)
	4.3 
(2.1-9.7)
	90 
(40-210)
	20 
(10-40)
	4.3 
(2.1-9.8)
	90 
(40-210)
	20 
(10-40)

	NY
	4.5 
(3.0-7.1)
	1000 
(700-1600)
	180 
(120-290)
	4.5 
(2.9-7.1)
	1000 
(700-1600)
	180 
(120-280)
	4.5 
(3.0-7.1)
	900 
(600-1500)
	170 
(110-270)
	4.5 
(2.9-7.1)
	900 
(600-1500)
	170
(110-270)
	4.5 
(2.9-7.1)
	900 
(600-1500)
	170 
(110-260)

	NC
	5.2 
(3.6-7.6)
	600 
(400-900)
	110 
(80-160)
	5.2 
(3.6-7.7)
	600 
(400-900)
	110 
(80-160)
	5.2 
(3.6-7.7)
	600 
(400-900)
	110 
(80-160)
	5.2 
(3.6-7.6)
	600 
(400-900)
	110
(80-170)
	5.1 
(3.5-7.6)
	600 
(400-900)
	110 
(80-170)

	ND
	4.7 
(2.7-8.5)
	50 
(30-90)
	10 
(10-20)
	4.7 
(2.8-8.4)
	50 
(30-90)
	10 
(10-20)
	4.7 
(2.8-8.5)
	50 
(30-90)
	10 
(0-20)
	4.6 
(2.7-8.2)
	50 
(30-80)
	10 
(0-10)
	4.6 
(2.8-8.2)
	40 
(30-80)
	10 
(0-10)

	OH
	4.8 
(3.3-6.8)
	700 
(500-900)
	120 
(80-170)
	4.9 
(3.4-6.9)
	700 
(500-900)
	120 
(80-170)
	4.8 
(3.3-6.9)
	600 
(400-900)
	110 
(80-160)
	4.8 
(3.3-6.8)
	600 
(400-900)
	110 
(80-160)
	4.8 
(3.3-6.8)
	600 
(400-900)
	110 
(80-160)

	OK
	4.9 
(2.9-9.4)
	200 
(100-500)
	40 
(30-80)
	5.0 
(2.9-9.5)
	200 
(100-500)
	40 
(30-80)
	5.0 
(2.9-9.4)
	200 
(100-400)
	40 
(20-80)
	5.0 
(2.9-9.5)
	200 
(100-500)
	40 
(20-80)
	4.9 
(2.9-9.4)
	200 
(100-500)
	40 
(20-80)

	OR
	4.1 
(2.4-6.7)
	200 
(100-300)
	30 
(20-50)
	4.1 
(2.4-6.7)
	200 
(100-300)
	30 
(20-50)
	4.1 
(2.4-6.7)
	200 
(100-300)
	30 
(20-50)
	4.1 
(2.4-6.7)
	200 
(100-300)
	30 
(20-50)
	4.1 
(2.4-6.9)
	200 
(100-300)
	30 
(20-50)

	PA
	4.6 
(3.1-6.8)
	600 
(400-900)
	110 
(80-170)
	4.6 
(3.1-6.8)
	600 
(400-900)
	110 
(70-160)
	4.6 
(3.1-6.8)
	600 
(400-900)
	110 
(70-160)
	4.6
(3.1-6.8)
	600 
(400-900)
	110 
(70-160)
	4.6 
(3.0-6.8)
	600 
(400-900)
	110 
(70-160)

	RI
	4.3 
(2.6-6.9)
	40 
(30-70)
	10 
(0-10)
	4.3 
(2.7-7.0)
	40 
(30-70)
	10 
(0-10)
	4.3 
(2.7-7.0)
	40 
(30-70)
	10 
(0-10)
	4.3
(2.7-6.9)
	50 
(30-70)
	10 
(10-10)
	4.3 
(2.7-6.9)
	40 
(30-70)
	10 
(0-10)

	SC
	5.5 
(4.1-7.5)
	300 
(200-400)
	60 
(40-80)
	5.5 
(4.1-7.5)
	300 
(200-400)
	60 
(40-80)
	5.5 
(4.1-7.5)
	300 
(200-400)
	60 
(40-80)
	5.5 
(4.0-7.5)
	300 
(200-400)
	60 
(40-80)
	5.4 
(3.9-7.5)
	300 
(200-400)
	60 
(40-80)

	SD
	4.8 
(2.6-10.0)
	60 
(30-120)
	10 
(10-20)
	4.8 
(2.6-10.1)
	60 
(30-120)
	10 
(10-20)
	4.8 
(2.6-10.0)
	50 
(30-110)
	10 
(10-20)
	4.8 
(2.6-9.9)
	50 
(30-110)
	10 
(10-20)
	4.8 
(2.6-9.8)
	50 
(30-110)
	10 
(10-20)

	TN
	5.0 
(3.5-7.0)
	400 
(300-600)
	70 
(50-100)
	5.0 
(3.5-7.0)
	400 
(300-600)
	70 
(50-100)
	5.0 
(3.5-7.0)
	400 
(300-600)
	70 
(50-100)
	4.9 
(3.4-7.0)
	400 
(300-600)
	70 
(50-100)
	4.9 
(3.3-7.0)
	400 
(300-600)
	70 
(50-100)

	TX
	4.4 
(2.7-7.3)
	1700 
(1000-2800)
	300 
(190-500)
	4.4 
(2.7-7.3)
	1700 
(1000-2800)
	300 
(190-500)
	4.4 
(2.7-7.3)
	1600 
(1000-2700)
	290 
(180-490)
	4.4 
(2.7-7.3)
	1600 
(1000-2700)
	300 
(180-490)
	4.4 
(2.7-7.4)
	1700 
(1100-2900)
	310 
(190-520)

	UT
	4.0 
(2.3-6.4)
	200 
(100-300)
	30 
(20-50)
	4.0 
(2.3-6.4)
	200 
(100-300)
	30 
(20-50)
	4.0 
(2.3-6.4)
	200 
(100-300)
	30 
(20-50)
	4.0 
(2.4-6.4)
	200 
(100-300)
	30 
(20-50)
	4.0 
(2.3-6.4)
	200 
(100-300)
	30 
(20-50)

	VT
	4.0 
(2.5-6.0)
	20 
(10-30)
	0 
(0-10)
	4.1 
(2.5-6.0)
	20 
(10-30)
	0 
(0-10)
	4.0 
(2.5-6.1)
	20 
(10-30)
	0 
(0-10)
	4.1 
(2.5-6.1)
	20 
(10-30)
	0 
(0-10)
	4.1 
(2.5-6.1)
	20 
(10-30)
	0 
(0-10)

	VA
	5.0 
(3.4-7.2)
	500 
(300-700)
	90 
(60-130)
	4.9 
(3.4-7.2)
	500 
(300-700)
	90 
(60-130)
	5.0 
(3.4-7.3)
	500 
(300-700)
	80 
(60-120)
	4.9 
(3.4-7.2)
	500 
(300-700)
	80 
(60-120)
	4.9 
(3.3-7.2)
	500 
(300-700)
	80 
(60-120)

	WA
	4.1 
(2.5-7.0)
	400 
(200-600)
	60 
(40-110)
	4.1 
(2.5-7.0)
	400 
(200-600)
	60 
(40-110)
	4.1 
(2.5-7.0)
	300 
(200-600)
	60 
(40-100)
	4.1 
(2.4-7.0)
	300 
(200-600)
	60 
(40-110)
	4.1 
(2.4-7.0)
	300 
(200-600)
	60 
(40-110)

	WV
	4.1 
(2.6-6.1)
	80 
(50-110)
	10 
(10-20)
	4.2 
(2.6-6.1)
	80 
(50-110)
	10 
(10-20)
	4.2 
(2.6-6.1)
	70 
(50-110)
	10 
(10-20)
	4.1 
(2.6-6.1)
	70 
(40-100)
	10 
(10-20)
	4.2 
(2.6-6.1)
	70 
(40-100)
	10 
(10-20)

	WI
	4.5 
(2.9-6.9)
	300 
(200-400)
	60 
(40-80)
	4.5 
(2.9-6.9)
	300 
(200-400)
	50 
(30-80)
	4.5 
(2.9-6.9)
	300 
(200-400)
	50
(30-70)
	4.5 
(2.9-6.8)
	300 
(200-400)
	50 
(30-80)
	4.4
(2.9-6.8)
	300 
(200-400)
	50 
(30-70)

	WY
	4.1 
(2.4-7.1)
	100 
(0-100)
	10 
(0-20)
	4.1 
(2.4-6.9)
	30 
(20-50)
	0 
(0-10)
	4.1 
(2.4-6.9)
	30 
(10-40)
	0 
(0-10)
	4.1 
(2.4-7.0)
	30 
(10-40)
	0 
(0-10)
	4.1 
(2.4-7.0)
	20 
(10-40)
	0 
(0-10)

	CI, confidence interval; Dis, disease; Inf, infection; No, number; Prev, prevalence

	Note: We rounded the number of infections to the nearest 100, unless the point estimate was <100, in which case we rounded to the nears 10; we rounded the number of disease cases to the nearest 10. Due to rounding schemes, some confidence intervals may overlap the point estimate. 



	Supplemental Table 3. National and state-specific cCMV infection prevalence per 1,000 live births, estimated number of infections, and estimated number of symptomatic cases, adjusted by maternal age group, 2018–2022 

	
	2018
	2019
	2020
	2021
	2022

	
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)
	Prev
(95% CI)
	No. inf
(95% CI)
	No. dis
(95% CI)

	US
	4.4 
(3.1-6.7)
	16800 
(11800-25500)
	3020 
(2130-4590)
	4.4 
(3.1-6.7)
	16500 
(11600-25100)
	2960 
(2080-4530)
	4.4 
(3.0-6.7)
	15800 
(11000-24200)
	2840 
(1980-4360)
	4.3 
(3.0-6.7)
	15800 
(10900-24500)
	2840 
(1970-4410)
	4.3 
(3.0-6.7)
	15700 
(10900-24500)
	2830 
(1950-4410)

	AL
	4.9 
(3.7-6.9)
	300 
(200-400)
	50 
(40-70)
	4.9 
(3.6-6.9)
	300 
(200-400)
	50 
(40-70)
	4.8 
(3.6-6.9)
	300 
(200-400)
	50 
(40-70)
	4.8 
(3.5-6.9)
	300 
(200-400)
	50 
(40-70)
	4.7 
(3.5-6.9)
	300 
(200-400)
	50 
(40-70)

	AK
	4.5 
(3.2-6.7)
	50 
(40-70)
	10 
(10-10)
	4.5 
(3.2-6.7)
	50 
(40-70)
	10 
(10-10)
	4.5 
(3.2-6.7)
	50 
(30-70)
	10 
(10-10)
	4.5 
(3.2-6.7)
	50 
(30-70)
	10 
(10-10)
	4.4 
(3.1-6.7)
	50 
(30-70)
	10 
(10-10)

	AZ
	4.6 
(3.3-6.8)
	400 
(300-500)
	70 
(50-100)
	4.6 
(3.3-6.8)
	400 
(300-500)
	70 
(50-100)
	4.5 
(3.2-6.8)
	300 
(200-500)
	60 
(40-90)
	4.5 
(3.2-6.7)
	300 
(200-500)
	60 
(40-90)
	4.4 
(3.1-6.7)
	300 
(200-500)
	60 
(40-90)

	AR
	5.0 
(3.8-7.1)
	200 
(100-300)
	30 
(30-50)
	5.0 
(3.8-7.0)
	200 
(100-300)
	30 
(30-50)
	5.0 
(3.8-7.0)
	200 
(100-200)
	30 
(20-40)
	5.0 
(3.7-7.0)
	200 
(100-300)
	30 
(20-50)
	4.9 
(3.7-7.0)
	200 
(100-200)
	30 
(20-40)

	CA
	4.2 
(2.8-6.6)
	1900 
(1300-3000)
	340 
(230-540)
	4.1 
(2.8-6.6)
	1800 
(1200-2900)
	330 
(220-530)
	4.1 
(2.7-6.6)
	1700 
(1100-2800)
	310
(210-500)
	4.1 
(2.7-6.6)
	1700 
(1100-2800)
	310 
(200-500)
	4.0 
(2.7-6.6)
	1700 
(1100-2800)
	300 
(200-500)

	CO
	4.3 
(2.9-6.7)
	300 
(200-400)
	50 
(30-80)
	4.2 
(2.9-6.7)
	300 
(200-400)
	50 
(30-80)
	4.2 
(2.9-6.7)
	300 
(200-400)
	50 
(30-70)
	4.2 
(2.8-6.6)
	300 
(200-400)
	50 
(30-80)
	4.1 
(2.8-6.6)
	300 
(200-400)
	50 
(30-70)

	CT
	4.0 
(2.6-6.6)
	100 
(100-200)
	20 
(20-40)
	4.0 
(2.6-6.6)
	100 
(100-200)
	20 
(20-40)
	4.0 
(2.6-6.6)
	100 
(100-200)
	20 
(20-40)
	3.9 
(2.5-6.6)
	100 
(100-200)
	30 
(20-40)
	3.9 
(2.4-6.5)
	100 
(100-200)
	20 
(20-40)

	DE
	4.4 
(3.1-6.7)
	50 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.6)
	50 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.7)
	40 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.7)
	50 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.7)
	50 
(30-70)
	10 
(10-10)

	DC
	4.1 
(2.7-6.7)
	40 
(20-60)
	10 
(0-10)
	4.0 
(2.6-6.6)
	40 
(20-60)
	10 
(0-10)
	4.0 
(2.6-6.6)
	40 
(20-60)
	10 
(0-10)
	3.9 
(2.5-6.6)
	30 
(20-60)
	10 
(0-10)
	3.9 
(2.4-6.6)
	30 
(20-50)
	10 
(0-10)

	FL
	4.4 
(3.1-6.7)
	1000 
(700-1500)
	170 
(120-270)
	4.4 
(3.0-6.7)
	1000 
(700-1500)
	170 
(120-260)
	4.3 
(3.0-6.7)
	900 
(600-1400)
	160 
(110-250)
	4.3 
(2.9-6.7)
	900 
(600-1400)
	170 
(110-260)
	4.2 
(2.9-6.6)
	900 
(600-1500)
	170 
(120-270)

	GA
	4.6 
(3.3-6.8)
	600 
(400-900)
	100 
(80-150)
	4.6 
(3.3-6.8)
	600 
(400-900)
	100 
(80-150)
	4.6 
(3.3-6.8)
	600 
(400-800)
	100 
(70-150)
	4.5 
(3.2-6.8)
	600 
(400-800)
	100 
(70-150)
	4.5 
(3.2-6.8)
	600 
(400-900)
	100 
(70-150)

	HI
	4.3 
(3.0-6.7)
	70 
(50-110)
	10 
(10-20)
	4.3 
(3.0-6.6)
	70 
(50-110)
	10 
(10-20)
	4.3 
(2.9-6.6)
	70 
(50-100)
	10 
(10-20)
	4.2 
(2.8-6.6)
	70 
(40-100)
	10 
(10-20)
	4.2 
(2.8-6.6)
	60 
(40-100)
	10 
(10-20)

	ID
	4.6 
(3.4-6.8)
	100 
(70-140)
	20 
(10-30)
	4.6 
(3.3-6.7)
	100 
(70-150)
	20 
(10-30)
	4.6 
(3.3-6.7)
	100 
(70-140)
	20 
(10-30)
	4.5 
(3.2-6.7)
	100 
(70-150)
	20 
(10-30)
	4.5 
(3.2-6.7)
	100 
(70-150)
	20 
(10-30)

	IL
	4.3 
(3.0-6.7)
	600 
(400-1000)
	110 
(80-170)
	4.3 
(2.9-6.7)
	600 
(400-900)
	110 
(70-170)
	4.2 
(2.9-6.7)
	600 
(400-900)
	100 
(70-160)
	4.2 
(2.8-6.6)
	600 
(400-900)
	100 
(70-160)
	4.2 
(2.8-6.6)
	500 
(400-900)
	100 
(60-150)

	IN
	4.7 
(3.5-6.8)
	400 
(300-600)
	70 
(50-100)
	4.7 
(3.4-6.8)
	400 
(300-600)
	70 
(50-100)
	4.6 
(3.4-6.8)
	400 
(300-500)
	70 
(50-100)
	4.6 
(3.3-6.8)
	400 
(300-500)
	70 
(50-100)
	4.6 
(3.3-6.8)
	400 
(300-500)
	70 
(50-100)

	IA
	4.4 
(3.2-6.6)
	200 
(100-200)
	30 
(20-40)
	4.4 
(3.1-6.6)
	200 
(100-200)
	30 
(20-40)
	4.4 
(3.1-6.6)
	200 
(100-200)
	30 
(20-40)
	4.3 
(3.0-6.6)
	200 
(100-200)
	30 
(20-40)
	4.3 
(3.0-6.6)
	200 
(100-200)
	30 
(20-40)

	KS
	4.6 
(3.3-6.8)
	200 
(100-200)
	30 
(20-40)
	4.6 
(3.3-6.8)
	200 
(100-200)
	30 
(20-40)
	4.6 
(3.3-6.8)
	200 
(100-200)
	30 
(20-40)
	4.5 
(3.2-6.7)
	200 
(100-200)
	30 
(20-40)
	4.5 
(3.2-6.7)
	200 
(100-200)
	30 
(20-40)

	KY
	4.9
(3.6-7.0)
	300 
(200-400)
	50 
(40-70)
	4.9 
(3.6-6.9)
	300 
(200-400)
	50 
(30-70)
	4.8 
(3.6-6.9)
	200 
(200-400)
	40 
(30-60)
	4.8
 (3.5-6.9)
	200 
(200-400)
	40 
(30-60)
	4.7 
(3.5-6.9)
	200 
(200-400)
	40 
(30-60)

	LA
	4.8 
(3.6-6.9)
	300 
(200-400)
	50 
(40-70)
	4.8 
(3.5-6.9)
	300 
(200-400)
	50 
(40-70)
	4.8 
(3.5-6.9)
	300 
(200-400)
	50 
(40-70)
	4.8 
(3.5-6.9)
	300 
(200-400)
	50 
(40-70)
	4.7 
(3.5-6.9)
	300 
(200-400)
	50 
(40-70)

	ME
	4.3 
(3.0-6.6)
	50 
(40-80)
	10 
(10-10)
	4.3 
(2.9-6.6)
	50 
(30-80)
	10 
(10-10)
	4.2 
(2.9-6.6)
	50 
(30-80)
	10 
(10-10)
	4.2 
(2.8-6.6)
	50 
(30-80)
	10 
(10-10)
	4.1 
(2.8-6.5)
	50 
(30-80)
	10 
(10-10)

	MD
	4.1 
(2.8-6.6)
	300 
(200-500)
	50 
(40-80)
	4.1 
(2.8-6.6)
	300 
(200-500)
	50 
(30-80)
	4.1 
(2.7-6.6)
	300 
(200-500)
	50 
(30-80)
	4.1 
(2.7-6.6)
	300 
(200-500)
	50 
(30-80)
	4.0 
(2.7-6.6)
	300 
(200-500)
	50 
(30-80)

	MA
	3.9 
(2.5-6.6)
	300 
(200-500)
	50 
(30-80)
	3.9 
(2.4-6.6)
	300 
(200-500)
	50 
(30-80)
	3.8 
(2.4-6.6)
	300 
(200-400)
	50 
(30-80)
	3.8 
(2.4-6.6)
	300 
(200-500)
	50 
(30-80)
	3.8 
(2.4-6.6)
	300 
(200-400)
	50 
(30-80)

	MI
	4.4 
(3.2-6.7)
	500 
(300-700)
	90 
(60-130)
	4.4 
(3.1-6.7)
	500 
(300-700)
	90
(60-130)
	4.4 
(3.1-6.7)
	500 
(300-700)
	80 
(60-120)
	4.3 
(3.0-6.6)
	500 
(300-700)
	80 
(60-130)
	4.3 
(3.0-6.6)
	400 
(300-700)
	80 
(50-120)

	MN
	4.1 
(2.7-6.5)
	300 
(200-400)
	50 
(30-80)
	4.1
(2.7-6.5)
	300 
(200-400)
	50 
(30-80)
	4.0 
(2.7-6.5)
	300 
(200-400)
	50 
(30-70)
	4.0 
(2.6-6.5)
	300 
(200-400)
	50 
(30-80)
	4.0 
(2.6-6.5)
	300 
(200-400)
	50 
(30-70)

	MS
	5.1 
(3.8-7.0)
	200 
(100-300)
	30 
(30-50)
	5.0 
(3.8-7.0)
	200 
(100-300)
	30 
(30-50)
	5.0 
(3.8-7.0)
	200 
(100-200)
	30 
(20-40)
	5.0 
(3.7-7.0)
	200 
(100-200)
	30 
(20-40)
	5.0 
(3.7-7.0)
	200 
(100-200)
	30 
(20-40)

	MO
	4.6 
(3.4-6.8)
	300 
(200-500)
	60 
(40-90)
	4.6 
(3.3-6.8)
	300 
(200-500)
	60 
(40-90)
	4.6 
(3.3-6.8)
	300 
(200-500)
	60 
(40-80)
	4.5 
(3.2-6.7)
	300 
(200-500)
	60 
(40-80)
	4.5 
(3.2-6.7)
	300 
(200-500)
	60 
(40-80)

	MT
	4.5 
(3.2-6.7)
	50 
(40-80)
	10 
(10-10)
	4.5 
(3.2-6.7)
	50 
(40-70)
	10 
(10-10)
	4.4 
(3.1-6.7)
	50 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.6)
	50 
(30-70)
	10 
(10-10)
	4.3
(3.0-6.6)
	50 
(30-70)
	10 
(10-10)

	NE
	4.4 
(3.1-6.6)
	100 
(100-200)
	20 
(10-30)
	4.3 
(3.1-6.6)
	100 
(100-200)
	20 
(10-30)
	4.3 
(3.0-6.6)
	100 
(100-200)
	20 
(10-30)
	4.3 
(3.0-6.6)
	100 
(100-200)
	20 
(10-30)
	4.3 
(3.0-6.6)
	100 
(100-200)
	20 
(10-30)

	NV
	4.5 
(3.2-6.8)
	200 
(100-200)
	30 
(20-40)
	4.5 
(3.2-6.7)
	200 
(100-200)
	30 
(20-40)
	4.4 
(3.1-6.7)
	100 
(100-200)
	30 
(20-40)
	4.4 
(3.1-6.6)
	100 
(100-200)
	30 
(20-40)
	4.3 
(3.0-6.6)
	100 
(100-200)
	30 
(20-40)

	NH
	4.1 
(2.7-6.6)
	50 
(30-80)
	10 
(10-10)
	4.0 
(2.7-6.5)
	50 
(30-80)
	10 
(10-10)
	4.0 
(2.6-6.5)
	50 
(30-80)
	10 
(10-10)
	3.9 
(2.5-6.5)
	50 
(30-80)
	10 
(10-10)
	3.9 
(2.5-6.5)
	50 
(30-80)
	10 
(10-10)

	NJ
	4.0 
(2.6-6.6)
	400 
(300-700)
	70 
(50-120)
	4.0
(2.6-6.6)
	400 
(300-700)
	70 
(50-120)
	3.9 
(2.5-6.6)
	400 
(200-600)
	70 
(40-120)
	3.9 
(2.5-6.6)
	400 
(300-700)
	70 
(50-120)
	3.9 
(2.5-6.6)
	400 
(300-700)
	70 
(50-120)

	NM
	4.8
(3.6-6.9)
	100 
(100-200)
	20 
(10-30)
	4.8 
(3.5-6.9)
	100 
(100-200)
	20 
(10-30)
	4.8 
(3.5-6.9)
	100 
(80-150)
	20 
(10-30)
	4.7
(3.4-6.9)
	100 
(70-150)
	20 
(10-30)
	4.7 
(3.4-6.9)
	100 
(70-150)
	20 
(10-30)

	NY
	4.1 
(2.8-6.6)
	900 
(600-1500)
	170 
(110-270)
	4.1 
(2.7-6.6)
	900 
(600-1500)
	160
(110-260)
	4.1 
(2.7-6.6)
	900 
(600-1400)
	150 
(100-250)
	4.0 
(2.6-6.6)
	800 
(600-1400)
	150 
(100-250)
	4.0 
(2.6-6.6)
	800 
(500-1400)
	150 
(100-250)

	NC
	4.6 
(3.3-6.8)
	500 
(400-800)
	100 
(70-150)
	4.5 
(3.3-6.8)
	500 
(400-800)
	100 
(70-150)
	4.5 
(3.2-6.8)
	500 
(400-800)
	90 
(70-140)
	4.4 
(3.1-6.8)
	500 
(400-800)
	100 
(70-150)
	4.4 
(3.1-6.7)
	500 
(400-800)
	100 
(70-150)

	ND
	4.4 
(3.1-6.5)
	50 
(30-70)
	10 
(10-10)
	4.3 
(3.1-6.6)
	50 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.5)
	40 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.5)
	40 
(30-70)
	10 
(10-10)
	4.3 
(3.0-6.6)
	40 
(30-60)
	10 
(10-10)

	OH
	4.6 
(3.3-6.8)
	600 
(400-900)
	110 
(80-160)
	4.6 
(3.3-6.8)
	600 
(400-900)
	110 
(80-160)
	4.5 
(3.2-6.8)
	600 
(400-900)
	100 
(70-160)
	4.5 
(3.2-6.7)
	600 
(400-900)
	100
(70-160)
	4.4 
(3.1-6.7)
	600 
(400-900)
	100 
(70-160)

	OK
	4.9 
(3.6-6.9)
	200 
(200-300)
	40 
(30-60)
	4.9 
(3.7-6.9)
	200 
(200-300)
	40 
(30-60)
	4.9 
(3.6-6.9)
	200 
(200-300)
	40 
(30-60)
	4.8 
(3.6-6.9)
	200 
(200-300)
	40 
(30-60)
	4.8 
(3.5-6.9)
	200 
(200-300)
	40 
(30-60)

	OR
	4.3 
(3.0-6.6)
	200 
(100-300)
	30 
(20-50)
	4.3 
(2.9-6.6)
	200 
(100-300)
	30 
(20-50)
	4.2 
(2.9-6.6)
	200 
(100-300)
	30 
(20-50)
	4.2 
(2.8-6.6)
	200 
(100-300)
	30 
(20-50)
	4.2 
(2.8-6.6)
	200 
(100-300)
	30 
(20-50)

	PA
	4.3 
(3-6.7)
	600 
(400-900)
	110 
(70-160)
	4.3 
(3.0-6.7)
	600 
(400-900)
	100 
(70-160)
	4.3 
(2.9-6.7)
	600 
(400-900)
	100 
(70-160)
	4.2 
(2.8-6.6)
	600 
(400-900)
	100 
(70-160)
	4.2 
(2.8-6.6)
	500 
(400-900)
	100
(70-160)

	RI
	4.2 
(2.9-6.6)
	40 
(30-70)
	10 
(10-10)
	4.2 
(2.8-6.6)
	40 
(30-70)
	10 
(10-10)
	4.1 
(2.8-6.6)
	40 
(30-70)
	10 
(10-10)
	4.1
(2.7-6.6)
	40 
(30-70)
	10 
(10-10)
	4.0 
(2.6-6.6)
	40 
(30-70)
	10 
(0-10)

	SC
	4.7 
(3.4-6.8)
	300 
(200-400)
	50 
(30-70)
	4.6 
(3.4-6.8)
	300 
(200-400)
	50 
(30-70)
	4.6 
(3.3-6.8)
	300
(200-400)
	50 
(30-70)
	4.5 
(3.2-6.8)
	300 
(200-400)
	50 
(30-70)
	4.5 
(3.2-6.8)
	300 
(200-400)
	50 
(30-70)

	SD
	4.5 
(3.2-6.6)
	50 
(40-80)
	10 
(10-10)
	4.4 
(3.2-6.6)
	50 
(40-80)
	10 
(10-10)
	4.4 
(3.2-6.6)
	50 
(30-70)
	10 
(10-10)
	4.4 
(3.1-6.6)
	50 
(40-80)
	10 
(10-10)
	4.4 
(3.1-6.6)
	50 
(30-70)
	10 
(10-10)

	TN
	4.8 
(3.5-6.9)
	400 
(300-600)
	70 
(50-100)
	4.7 
(3.5-6.9)
	400 
(300-600)
	70 
(50-100)
	4.7 
(3.4-6.9)
	400 
(300-500)
	70 
(50-100)
	4.6 
(3.4-6.8)
	400
(300-600)
	70 
(50-100)
	4.6 
(3.3-6.8)
	400 
(300-600)
	70 
(50-100)

	TX
	4.7 
(3.4-6.9)
	1800 
(1300-2600)
	320 
(230-470)
	4.6 
(3.3-6.8)
	1700 
(1300-2600)
	310 
(230-470)
	4.6 
(3.3-6.8)
	1700 
(1200-2500)
	310 
(220-450)
	4.5 
(3.3-6.8)
	1700 
(1200-2500)
	310 
(220-460)
	4.5 
(3.2-6.8)
	1800 
(1300-2600)
	320 
(230-480)

	UT
	4.4 
(3.2-6.6)
	200 
(200-300)
	40 
(30-60)
	4.4 
(3.1-6.6)
	200 
(100-300)
	40 
(30-60)
	4.4 
(3.1-6.5)
	200 
(100-300)
	40 
(30-50)
	4.3 
(3.1-6.5)
	200 
(100-300)
	40 
(30-50)
	4.3 
(3.1-6.5)
	200 
(100-300)
	40 
(30-50)

	VT
	4.2 
(2.8-6.6)
	20 
(20-40)
	0 
(0-10)
	4.1 
(2.8-6.6)
	20 
(10-40)
	0 
(0-10)
	4.1
(2.7-6.6)
	20 
(10-30)
	0 
(0-10)
	4.0 
(2.6-6.6)
	20 
(10-40)
	0 
(0-10)
	4.0 
(2.6-6.6)
	20 
(10-30)
	0 
(0-10)

	VA
	4.3 
(2.9-6.7)
	400 
(300-700)
	80
(50-120)
	4.3 
(2.9-6.7)
	400 
(300-600)
	70 
(50-120)
	4.2 
(2.9-6.7)
	400 
(300-600)
	70 
(50-110)
	4.2 
(2.8-6.6)
	400 
(300-600)
	70 
(50-110)
	4.1 
(2.8-6.6)
	400 
(300-600)
	70 
(50-110)

	WA
	4.2 
(2.9-6.6)
	400 
(200-600)
	70 
(40-100)
	4.2 
(2.9-6.6)
	400 
(200-600)
	60 
(40-100)
	4.1 
(2.8-6.6)
	300 
(200-500)
	60 
(40-100)
	4.1 
(2.8-6.6)
	300 
(200-600)
	60 
(40-100)
	4.1 
(2.7-6.6)
	300 
(200-500)
	60 
(40-100)

	WV
	5.0 
(3.8-7.0)
	90 
(70-130)
	20 
(10-20)
	5.0
(3.8-7.0)
	90 
(70-130)
	20 
(10-20)
	4.9 
(3.7-7.0)
	90 
(60-120)
	20 
(10-20)
	4.9 
(3.7-7.0)
	80 
(60-120)
	20 
(10-20)
	4.9 
(3.6-6.9)
	80 
(60-120)
	10 
(10-20)

	WI
	4.3 
(3.0-6.6)
	300 
(200-400)
	50 
(30-80)
	4.3 
(3.0-6.6)
	300 
(200-400)
	50 
(30-80)
	4.2 
(2.9-6.6)
	300 
(200-400)
	50 
(30-70)
	4.2 
(2.9-6.6)
	300
(200-400)
	50 
(30-70)
	4.1
(2.8-6.6)
	200 
(200-400)
	40 
(30-70)

	WY
	4.7 
(3.4-6.8)
	30 
(20-40)
	10 
(0-10)
	4.7 
(3.4-6.8)
	30 
(20-40)
	10 
(0-10)
	4.7 
(3.4-6.8)
	30 
(20-40)
	10 
(0-10)
	4.6 
(3.3-6.8)
	30 
(20-40)
	10 
(0-10)
	4.6 
(3.3-6.8)
	30 
(20-40)
	0 
(0-10)

	CI, confidence interval; Dis, disease; Inf, infection; No, number; Prev, prevalence

	Note: We rounded the number of infections to the nearest 100, unless the point estimate was <100, in which case we rounded to the nears 10; we rounded the number of disease cases to the nearest 10. Due to rounding schemes, some confidence intervals may overlap the point estimate. 





