**Supplemental Information**

**Evaluation of the Alphasense Optical Particle Counter (OPC-N2) and the Grimm Portable Aerosol Spectrometer (PAS-1.108)**

Sinan Sousan1, Kirsten Koehler2, Laura Hallett1, and Thomas M. Peters1

1Department of Occupational and Environmental Health, University of Iowa, Iowa City, Iowa, USA

2Environmental Health Sciences, Johns Hopkins Bloomberg School of Public Health, Baltimore, Maryland, USA

|  |
| --- |
| Table S1: Manufacturer-reported and measured sizes of monodispersed PSL particles. |
| **PSL size according to the manufacturer (µm)** | **OPC-N2****bin range diameter (µm)1** | **PAS-1.108** **bin range diameter (µm)1** | **APS/SMPS2****Median diameter (µm)1** | **APS/SMPS2****Mode diameter (µm)1** | **APS/SMPS2****Geometric Standard Deviation**  |
| 0.5 | 0.38-0.54 | 0.5-0.65 | 0.5 | 0.5 | 1.07 |
| 0.83 | 0.78-1.05 | 0.8-1.0 | 0.82 | 0.84 | 1.1 |
| 1.0 | 0.78-1.05 | 0.8-1.0 | 1.03 | 1.04 | 1.09 |
| 3.0 | 2.07-3.0 | 2.0-3.0 | 2.87 | 2.84 | 1.06 |
| 5.0 | 4.0-5.0 | 4.0-5.0 | 4.7 | 4.7 | 1.04 |
| 1Volumetric diameter |
| 2SMPS only for the 0.5 µm particle size.  |

|  |
| --- |
|   |
| A) Salt |
|  |
| B) Welding fume |
|  |
| C) ARD |
|  |
| Figure S1: Fractional number concentration by size measured for low and high concentrations for A) Salt; B) Welding fume; and C) ARD |

|  |
| --- |
|   |
| A) Salt |
|  |
| B) Welding fume |
|  |
| C) ARD |
|  |
| Figure S1: Fractional mass concentration by size measured for low and high concentrations for A) Salt; B) Welding fume; and C) ARD |